**RF2-3 Individual Ratings**

|  |  |  |
| --- | --- | --- |
| Single-Phase | | |
| Frequency | 50Hz | 60Hz |
| Apparent Power | 1.6kVA | 1.9kVA |
| Rated Power | 1.3kW | 1.56kW |
| Voltage | 230 | 230 |
| Efficiency @ 50% Load | 75.5% | 79.6% |
| Efficiency @ 75% Load | 79.89% | 81.9% |
| Efficiency @ 100% Load | 79.69% | 81.3% |
| Current | 6.02A | 7.22A |
| Torque | 5.2N.m | 6.24N.m |
| Motor Start Capability | 4kVA | 4.8kVA |
| Short Circuit Current | 18A | 21.6A |
| Total Harmonic Distortion (THD) | 5.75 | 5.75 |
| Voltage Transient | +0.0%/-6.0% | +0.0%/-6.0% |
| Transient Response Time | <0.01ms | <0.01ms |
| Frame Size | 132mm | 132mm |
| Shaft Coupling | V-Taper 2¼ inch per foot | V-Taper 2¼ inch per foot |
| Insulation Class | H | H |
| IP Rating | IP23 | IP23 |
|  |  |  |